### The right solution for any task:

# Laminate, parquet, LVT, SPC, wall and ceiling panels, mineral fiber panels — a diverse range of the highest quality

Maximum profile accuracy — the new TENONTEQ D-500 double-end profiler series

The **new HOMAG TENONTEQ D-500 | D-600 | D-800 double-end profilers** have a modular construction and impress with a more rigid and stable design. At LIGNA,visitors will be able to see our entry-level series, the **TENONTEQ D-500**, live in action in Hall 14 in the **"Components"** technology area.

This compact double-sided dimensioning machine impresses with its excellent processing quality and efficiency. As a cost-effective combined longitudinal/crosswise machine, it can trim longitudinal and crosswise profiles or create formatting, all in a wide variety of materials such as parquet, LVT, laminate, SPC or mineral fiber panels. The flexibility of the machine means that it can be used for wall and ceiling panels, as well as for all types of flooring (tongue and groove or click-loc profiles). It is also suitable for medium-sized construction companies who want to manufacture their own creative floor and wall coverings cost-effectively, quickly and independently.

The heavy machine weight ensures quiet operation, while high-frequency motors that can be swiveled precisely and flexible equipment ensure workpieces can be produced with maximum profile accuracy and precision. The machines can be controlled easily either by using the proven protection control, or intuitively via powerTouch.

Image source: HOMAG Group AG



Image:

TENONTEQ D-500 double-end profiler

**If you have any questions, please contact:**

**HOMAG Group AG**

Homagstrasse 3–5

72296 Schopfloch

Germany

www.homag.com

**Julia Weber**

Customer Communication Manager

Tel. +49 (0) 7443 13-2588

Fax +49 (0) 7443 13-8-2588

julia.weber@homag.com